Supplementary Table 4. Hazard ratios (95% confidence intervals) for all-cause mortality according to dialyzer surface area in 234,638 patients on maintenance hemodialysis, determined using a standard Cox proportional hazards regression model

	Group
	Unadjusted
	　
	Adjusted for basic factorsa
	　
	Adjusted for basic factors and dialysis-related factorsb
	　
	Adjusted for basic, dialysis-related, and nutrition/inflammation-related factorsc

	
	HR
	95% CI
	P-value
	　
	HR
	95% CI
	P-value
	　
	HR
	95% CI
	P-value
	　
	HR
	95% CI
	P-value

	S
	1.61
	1.57–1.65
	< 0.0001
	
	1.27
	1.24–1.30
	< 0.0001
	
	1.23
	1.23–1.29
	< 0.0001
	
	1.15
	1.12–1.19
	< 0.0001

	M
	1.00
	Reference
	–
	
	1.00
	Reference
	–
	
	1.00
	Reference
	–
	
	1.00
	Reference
	–

	L
	0.71
	0.69–0.72
	< 0.0001
	
	0.86
	0.84–0.88
	< 0.0001
	
	0.86
	0.84–0.89
	< 0.0001
	
	0.89 
	0.87–0.92
	< 0.0001

	XL
	0.44
	0.43–0.45
	< 0.0001
	　
	0.68
	0.66–0.70
	< 0.0001
	　
	0.70
	0.68–0.73
	< 0.0001
	　
	0.75 
	0.72–0.78
	< 0.0001



S group, small dialyzer surface area, <1.5 m2; M group, medium dialyzer surface area, 1.5 m2; L group, large dialyzer surface area, 1.6 to <2.0 m2; XL group, extra-large dialyzer surface area, ≥2.0 m2. aAdjusted for age, sex, duration of dialysis, presence or absence of diabetes, and cardiovascular disease. bAdjusted for clinicodemographic factors and dialysis-related factors, including Kt/V, β2-microglobulin level, ultrafiltration rate, dialysis time, and type of dialyzer. cAdjusted for clinicodemographic and dialysis-related factors, C-reactive protein, hemoglobin, normalized protein catabolic rate, serum albumin, body mass index, and simplified creatinine index. CI, confidence interval; HR, hazard ratio.

