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Supplementary Figure 1: Heat production, O2 consumption, CO2 production, respiratory quotient, CH4 production and activity during the heat stress challenge of pigs housed in an alternative (AHS, grey line) or conventional system (CONV, black line).
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