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Supplementary Figure 1. Raw PEEK chamber following extrusion printing. To correct for irregularities the surface was ground before experimental use.
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