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Figure SI1. Scheme of the homemade system for homogenous heating of tobacco. The cigarette is inserted into the copper tube, leaving the filter outside. The copper cylinder is heated using a heating coil at the desired temperature, which is controlled through the thermocouple inserted into the tobacco.
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