	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.075
	1.056
	1.013
	0.999
	0.989

	95% CI
	0.999-1.157
	1.004-1.110
	1.000-1.025
	0.983-1.016
	0.969-1.011

	p-value
	0.053
	0.035
	0.052
	0.925
	0.325

	LAG 1

	OR
	0.975
	0.981
	0.993
	1.002
	1.016

	95% CI
	0.894-1.062
	0.923-1.042
	0.979-1.008
	0.985-1.020
	0.991-1.042

	p-value
	0.557
	0.533
	0.371
	0.828
	0.213

	LAG 2

	OR
	0.984
	0.963
	0.996
	0.999
	0.976

	95% CI
	0.902-1.074
	0.907-1.023
	0.982-1.011
	0.981-1.016
	0.953-0.999

	p-value
	0.718
	0.224
	0.624
	0.873
	0.037

	LAG 3

	OR
	1.015
	1.024
	0.999
	1.002
	1.026

	95% CI
	0.929-1.110
	0.962-1.089
	0.984-1.014
	0.984-1.020
	1.004-1.049

	p-value
	0.739
	0.454
	0.878
	0.818
	0.022

	LAG 4

	OR
	1.021
	0.996
	1.002
	1.01
	0.996

	95% CI
	0.934-1.115
	0.937-1.060
	0.987-1.017
	0.993-1.027
	0.975-1.017

	p-value
	0.652
	0.908
	0.797
	0.266
	0.677

	LAG 5

	OR
	0.995
	1.015
	1.004
	0.994
	1.011

	95% CI
	0.912-1.085
	0.956-1.077
	0.989-1.019
	0.977-1.010
	0.990-1.033

	p-value
	0.905
	0.636
	0.593
	0.453
	0.31

	LAG 6

	OR
	0.989
	1.002
	0.998
	1
	0.987

	95% CI
	0.908-1.076
	0.944-1.064
	0.984-1.013
	0.981-1.019
	0.965-1.009

	p-value
	0.789
	0.944
	0.801
	0.997
	0.24

	LAG 7

	OR
	1.012
	0.996
	1.007
	1.007
	1.007

	95% CI
	0.943-1.085
	0.948-1.046
	0.994-1.020
	0.991-1.023
	0.987-1.026

	p-value
	0.749
	0.859
	0.278
	0.409
	0.504
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Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.




Table A2. Associations between the exposure to short-term pollutants and ischemic stroke incidence in female population.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.074
	1.065
	1.014
	1.001
	0.996

	95% CI
	0.993-1.160
	1.009-1.123
	1.000-1.027
	0.983-1.019
	0.975-1.018

	p-value
	0.073
	0.022
	0.043
	0.885
	0.724

	LAG 1

	OR
	0.951
	0.959
	0.996
	1.013
	1.001

	95% CI
	0.867-1.042
	0.900-1.023
	0.981-1.012
	0.995-1.032
	0.977-1.025

	p-value
	0.279
	0.204
	0.631
	0.153
	0.932

	LAG 2

	OR
	1.027
	0.993
	1.001
	1
	0.985

	95% CI
	0.936-1.126
	0.931-1.060
	0.986-1.017
	0.981-1.019
	0.962-1.010

	p-value
	0.577
	0.84
	0.862
	0.985
	0.241

	LAG 3

	OR
	0.993
	1.004
	0.992
	0.992
	1.020

	95% CI
	0.904-1.090
	0.941-1.071
	0.977-1.007
	0.972-1.012
	0.997-1.044

	p-value
	0.877
	0.908
	0.309
	0.41
	0.084

	LAG 4
	

	OR
	1.005
	0.982
	0.998
	1.012
	1.01

	95% CI
	0.917-1.103
	0.920-1.047
	0.983-1.013
	0.993-1.032
	0.987-1.032

	p-value
	0.911
	0.576
	0.76
	0.215
	0.397

	LAG 5

	OR
	0.941
	0.994
	0.998
	0.996
	0.985

	95% CI
	0.858-1.031
	0.932-1.059
	0.983-1.013
	0.978-1.014
	0.962-1.009

	p-value
	0.19
	0.84
	0.776
	0.638
	0.217

	LAG 6

	OR
	1.037
	1.027
	1.005
	0.994
	1.001

	95% CI
	0.947-1.135
	0.964-1.093
	0.990-1.021
	0.976-1.013
	0.978-1.025

	p-value
	0.431
	0.415
	0.506
	0.553
	0.941

	LAG 7

	OR
	0.984
	0.983
	1.005
	1.002
	1.004

	95% CI
	0.913-1.060
	0.932-1.037
	0.992-1.019
	0.986-1.020
	0.984-1.025

	p-value
	0.671
	0.531
	0.431
	0.776
	0.678


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.



Table A3. Associations between the exposure to short-term pollutants and ischemic stroke incidence in male population.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0
	
	
	
	
	

	OR
	1.054
	1.029
	1.006
	0.999
	0.994

	95% CI
	0.974-1.141
	0.974-1.087
	0.992-1.020
	0.981-1.018
	0.972-1.017

	p-value
	0.19
	0.308
	0.391
	0.924
	0.599

	LAG 1

	OR
	0.987
	1.007
	0.99
	0.988
	1.016

	95% CI
	0.900-1.082
	0.944-1.074
	0.975-1.006
	0.967-1.010
	0.989-1.045

	p-value
	0.78
	0.827
	0.205
	0.284
	0.253

	LAG 2

	OR
	0.977
	0.961
	0.995
	1.003
	0.974

	95% CI
	0.890-1.072
	0.900-1.027
	0.979-1.011
	0.983-1.023
	0.948-1.000

	p-value
	0.621
	0.241
	0.521
	0.773
	0.05

	LAG 3

	OR
	0.993
	1.003
	1.003
	1.003
	1.024

	95% CI
	0.902-1.093
	0.938-1.073
	0.988-1.020
	0.981-1.025
	0.998-1.050

	p-value
	0.882
	0.929
	0.677
	0.802
	0.07

	LAG 4

	OR
	1.004
	1.012
	1.004
	1.006
	0.982

	95% CI
	0.913-1.105
	0.948-1.082
	0.989-1.020
	0.986-1.027
	0.956-1.008

	p-value
	0.933
	0.714
	0.592
	0.539
	0.181

	LAG 5

	OR
	1.037
	1.021
	1.007
	0.993
	1.031

	95% CI
	0.944-1.139
	0.956-1.091
	0.991-1.023
	0.974-1.013
	1.005-1.058

	p-value
	0.451
	0.531
	0.382
	0.501
	0.019

	LAG 6

	OR
	0.963
	0.99
	0.99
	1.004
	0.982

	95% CI
	0.879-1.055
	0.929-1.056
	0.975-1.006
	0.985-1.024
	0.958-1.006

	p-value
	0.415
	0.763
	0.228
	0.66
	0.134

	LAG 7

	OR
	1.032
	1.012
	1.008
	1.009
	1.006

	95% CI
	0.957-1.114
	0.959-1.067
	0.994-1.022
	0.992-1.026
	0.985-1.027

	p-value
	0.411
	0.666
	0.275
	0.321
	0.581


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A4. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the study group of people younger than 65 years old.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	0.979
	1.01
	1.008
	0.994
	1.001

	95% CI
	0.887-1.080
	0.945-1.080
	0.992-1.025
	0.973-1.016
	0.979-1.023

	p-value
	0.667
	0.767
	0.343
	0.589
	0.934

	LAG 1

	OR
	0.984
	0.96
	0.985
	1.01
	1.022

	95% CI
	0.878-1.102
	0.886-1.041
	0.966-1.004
	0.989-1.032
	0.994-1.051

	p-value
	0.778
	0.325
	0.113
	0.339
	0.126

	LAG 2

	OR
	1.011
	1.037
	1
	0.979
	0.974

	95% CI
	0.904-1.132
	0.959-1.122
	0.981-1.019
	0.955-1.004
	0.944-1.006

	p-value
	0.844
	0.357
	0.994
	0.1
	0.106

	LAG 3

	OR
	0.963
	0.958
	1.001
	1.020
	1.004

	95% CI
	0.858-1.081
	0.884-1.039
	0.982-1.021
	0.998-1.042
	0.975-1.033

	p-value
	0.523
	0.304
	0.899
	0.076
	0.806

	LAG 4

	OR
	0.937
	0.975
	0.992
	0.992
	0.984

	95% CI
	0.835-1.052
	0.900-1.055
	0.974-1.012
	0.969-1.017
	0.953-1.015

	p-value
	0.273
	0.527
	0.433
	0.538
	0.3

	LAG 5

	OR
	1.035
	1.034
	1.002
	1.009
	1.028

	95% CI
	0.927-1.156
	0.958-1.116
	0.983-1.021
	0.988-1.030
	0.999-1.058

	p-value
	0.538
	0.395
	0.844
	0.391
	0.057

	LAG 6

	OR
	0.994
	0.992
	0.991
	0.995
	0.986

	95% CI
	0.891-1.108
	0.918-1.071
	0.972-1.009
	0.974-1.016
	0.958-1.015

	p-value
	0.908
	0.83
	0.329
	0.614
	0.351

	LAG 7

	OR
	1.047
	1.025
	1.014
	1.022
	1.007

	95% CI
	0.957-1.145
	0.962-1.092
	0.997-1.030
	1.004-1.041
	0.982-1.033

	p-value
	0.318
	0.442
	0.107
	0.015
	0.572


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A5. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the study group of people older than 65 years old.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.091
	1.068
	1.012
	1.005
	0.989

	95% CI
	1.013-1.176
	1.015-1.125
	1.000-1.025
	0.989-1.022
	0.968-1.011

	p-value
	0.021
	0.012
	0.059
	0.529
	0.339

	LAG 1

	OR
	0.965
	0.978
	0.995
	0.998
	1.004

	95% CI
	0.884-1.053
	0.920-1.040
	0.981-1.010
	0.979-1.017
	0.980-1.030

	p-value
	0.418
	0.484
	0.526
	0.809
	0.726

	LAG 2

	OR
	0.982
	0.958
	0.997
	1.006
	0.984

	95% CI
	0.898-1.074
	0.901-1.020
	0.982-1.012
	0.988-1.024
	0.960-1.007

	p-value
	0.691
	0.179
	0.675
	0.52
	0.176

	LAG 3

	OR
	1.024
	1.031
	0.999
	0.994
	1.027

	95% CI
	0.935-1.121
	0.968-1.099
	0.984-1.014
	0.976-1.012
	1.004-1.051

	p-value
	0.612
	0.337
	0.893
	0.477
	0.02

	LAG 4

	OR
	1.042
	1.005
	1.005
	1.016
	0.999

	95% CI
	0.953-1.140
	0.944-1.070
	0.990-1.020
	0.998-1.034
	0.978-1.021

	p-value
	0.366
	0.876
	0.528
	0.082
	0.952

	LAG 5

	OR
	0.959
	0.996
	1.002
	0.986
	1.006

	95% CI
	0.879-1.046
	0.937-1.059
	0.987-1.017
	0.968-1.004
	0.985-1.028

	p-value
	0.347
	0.907
	0.814
	0.131
	0.588

	LAG 6

	OR
	1.006
	1.016
	1.001
	1.006
	0.994

	95% CI
	0.924-1.096
	0.956-1.079
	0.986-1.015
	0.987-1.025
	0.973-1.016

	p-value
	0.888
	0.614
	0.916
	0.562
	0.612

	LAG 7

	OR
	0.993
	0.988
	1.003
	0.994
	1.001

	95% CI
	0.925-1.065
	0.940-1.039
	0.991-1.017
	0.978-1.011
	0.982-1.021

	p-value
	0.835
	0.649
	0.6
	0.496
	0.893


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A6. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the study group of people younger than 75 years old.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.071
	1.049
	1.015
	1.004
	0.974

	95% CI
	0.989-1.159
	0.993-1.107
	1.001-1.029
	0.987-1.022
	0.952-0.997

	p-value
	0.09
	0.085
	0.038
	0.621
	0.025

	LAG 1

	OR
	0.999
	0.998
	0.994
	1.006
	1.034

	95% CI
	0.910-1.096
	0.935-1.066
	0.979-1.010
	0.987-1.024
	1.008-1.061

	p-value
	0.978
	0.959
	0.49
	0.546
	0.009

	LAG 2

	OR
	0.977
	0.993
	0.998
	0.991
	0.981

	95% CI
	0.890-1.074
	0.930-1.061
	0.982-1.014
	0.971-1.011
	0.956-1.006

	p-value
	0.634
	0.832
	0.782
	0.385
	0.139

	LAG 3

	OR
	1.027
	1.009
	1.002
	1.007
	1.004

	95% CI
	0.935-1.128
	0.945-1.077
	0.986-1.018
	0.986-1.028
	0.980-1.028

	p-value
	0.577
	0.793
	0.836
	0.497
	0.772

	LAG 4

	OR
	1.003
	1.017
	1.002
	1.001
	1.011

	95% CI
	0.913-1.101
	0.952-1.086
	0.986-1.018
	0.982-1.021
	0.985-1.037

	p-value
	0.955
	0.62
	0.817
	0.889
	0.411

	LAG 5

	OR
	1.042
	1.022
	1.003
	1.002
	1.017

	95% CI
	0.949-1.145
	0.957-1.090
	0.988-1.019
	0.983-1.021
	0.991-1.042

	p-value
	0.387
	0.523
	0.677
	0.851
	0.198

	LAG 6

	OR
	0.938
	0.973
	0.993
	0.992
	0.979

	95% CI
	0.854-1.030
	0.911-1.039
	0.977-1.009
	0.972-1.012
	0.956-1.003

	p-value
	0.178
	0.407
	0.379
	0.443
	0.093

	LAG 7

	OR
	1.041
	1.014
	1.014
	1.013
	1.009

	95% CI
	0.964-1.124
	0.961-1.070
	1.000-1.028
	0.996-1.031
	0.988-1.029

	p-value
	0.304
	0.601
	0.048
	0.124
	0.417


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A7. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the study group of people older than 75 years old.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.035
	1.032
	1.001
	1.001
	1.012

	95% CI
	0.958-1.117
	0.979-1.089
	0.988-1.015
	0.982-1.020
	0.990-1.035

	p-value
	0.383
	0.237
	0.838
	0.929
	0.286

	LAG 1

	OR
	0.965
	0.968
	0.994
	0.999
	0.985

	95% CI
	0.882-1.056
	0.908-1.031
	0.979-1.010
	0.979-1.019
	0.959-1.011

	p-value
	0.437
	0.311
	0.466
	0.889
	0.252

	LAG 2

	OR
	0.988
	0.959
	0.997
	1.005
	0.978

	95% CI
	0.903-1.082
	0.900-1.022
	0.982-1.012
	0.986-1.024
	0.953-1.004

	p-value
	0.799
	0.196
	0.7
	0.615
	0.093

	LAG 3

	OR
	1.005
	1.023
	1
	0.991
	1.039

	95% CI
	0.916-1.103
	0.959-1.092
	0.985-1.015
	0.970-1.012
	1.014-1.065

	p-value
	0.908
	0.489
	0.998
	0.375
	0.002

	LAG 4

	OR
	1.029
	0.985
	1.001
	1.017
	0.987

	95% CI
	0.939-1.127
	0.924-1.051
	0.986-1.017
	0.996-1.037
	0.963-1.012

	p-value
	0.547
	0.649
	0.861
	0.107
	0.303

	LAG 5

	OR
	0.941
	0.999
	1.001
	0.988
	1.002

	95% CI
	0.860-1.030
	0.937-1.064
	0.986-1.016
	0.968-1.008
	0.978-1.026

	p-value
	0.185
	0.964
	0.911
	0.223
	0.884

	LAG 6

	OR
	1.043
	1.029
	1.002
	1.005
	1.003

	95% CI
	0.955-1.140
	0.965-1.096
	0.986-1.017
	0.986-1.024
	0.979-1.027

	p-value
	0.347
	0.383
	0.844
	0.598
	0.828

	LAG 7

	OR
	0.982
	0.982
	0.997
	0.994
	0.997

	95% CI
	0.913-1.056
	0.932-1.034
	0.983-1.010
	0.976-1.012
	0.977-1.018

	p-value
	0.628
	0.488
	0.642
	0.536
	0.795


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A8. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the spring
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.091
	1.094
	0.998
	0.877
	0.908

	95% CI
	0.775-1.537
	0.880-1.360
	0.967-1.030
	0.768-1.000
	0.078-10.632

	p-value
	0.617
	0.42
	0.897
	0.05
	0.939

	LAG 1

	OR
	1.332
	1.056
	1.008
	1.106
	2.51

	95% CI
	0.934-1.900
	0.843-1.322
	0.976-1.042
	0.953-1.284
	0.150-42.033

	p-value
	0.113
	0.635
	0.619
	0.186
	0.522

	LAG 2

	OR
	0.652
	0.818
	0.987
	0.999
	0.141

	95% CI
	0.456-0.933
	0.655-1.022
	0.955-1.020
	0.863-1.156
	0.008-2.410

	p-value
	0.019
	0.077
	0.428
	0.991
	0.176

	LAG 3

	OR
	1.125
	0.995
	0.971
	0.953
	0.319

	95% CI
	0.821-1.541
	0.804-1.233
	0.940-1.004
	0.826-1.100
	0.021-4.830

	p-value
	0.464
	0.966
	0.084
	0.512
	0.41

	LAG 4

	OR
	0.847
	0.934
	1
	1.037
	1.129

	95% CI
	0.621-1.155
	0.757-1.152
	0.969-1.033
	0.899-1.197
	0.072-17.742

	p-value
	0.294
	0.523
	0.976
	0.614
	0.931

	LAG 5

	OR
	0.905
	0.869
	1
	0.926
	1.212

	95% CI
	0.660-1.242
	0.702-1.076
	0.968-1.034
	0.800-1.073
	0.075-19.591

	p-value
	0.536
	0.198
	0.985
	0.306
	0.892

	LAG 6

	OR
	1.305
	1.18
	0.994
	1.137
	1.829

	95% CI
	0.963-1.769
	0.962-1.446
	0.962-1.027
	0.984-1.314
	0.144-23.226

	p-value
	0.086
	0.111
	0.713
	0.081
	0.642

	LAG 7

	OR
	0.927
	1.025
	1.023
	1.005
	1.972

	95% CI
	0.723-1.188
	0.872-1.205
	0.994-1.053
	0.888-1.137
	0.236-16.516

	p-value
	0.548
	0.767
	0.122
	0.943
	0.531


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A9. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the summer.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.218
	1.02
	1.016
	1.006
	0.995

	95% CI
	0.789-1.881
	0.801-1.298
	0.984-1.049
	0.967-1.047
	0.965-1.026

	p-value
	0.373
	0.873
	0.33
	0.768
	0.741

	LAG 1

	OR
	0.631
	1.055
	0.987
	0.993
	1.019

	95% CI
	0.389-1.024
	0.799-1.392
	0.951-1.025
	0.953-1.035
	0.981-1.059

	p-value
	0.062
	0.706
	0.494
	0.744
	0.331

	LAG 2

	OR
	0.863
	0.839
	0.998
	1.02
	0.957

	95% CI
	0.527-1.413
	0.635-1.110
	0.962-1.035
	0.980-1.061
	0.924-0.990

	p-value
	0.558
	0.219
	0.899
	0.333
	0.012

	LAG 3

	OR
	0.785
	1.006
	1.004
	0.974
	1.037

	95% CI
	0.476-1.295
	0.750-1.348
	0.968-1.041
	0.933-1.018
	1.008-1.067

	p-value
	0.343
	0.971
	0.838
	0.248
	0.013

	LAG 4

	OR
	1.129
	0.923
	0.982
	1.008
	1

	95% CI
	0.678-1.878
	0.692-1.231
	0.947-1.019
	0.965-1.052
	0.973-1.027

	p-value
	0.641
	0.584
	0.346
	0.717
	0.979

	LAG 5

	OR
	0.795
	0.936
	0.996
	0.993
	1.007

	95% CI
	0.473-1.336
	0.695-1.262
	0.960-1.035
	0.959-1.029
	0.981-1.034

	p-value
	0.386
	0.666
	0.852
	0.709
	0.596

	LAG 6

	OR
	1.337
	0.981
	1.004
	1.028
	0.999

	95% CI
	0.790-2.263
	0.726-1.326
	0.968-1.043
	0.994-1.063
	0.970-1.030

	p-value
	0.279
	0.899
	0.817
	0.106
	0.972

	LAG 7

	OR
	1.022
	1.135
	1.011
	1
	0.998

	95% CI
	0.645-1.618
	0.873-1.474
	0.977-1.045
	0.968-1.033
	0.972-1.026

	p-value
	0.927
	0.344
	0.542
	0.998
	0.905


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A10. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the autumn.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.055
	1.041
	1.007
	1
	0.970

	95% CI
	0.913-1.219
	0.951-1.139
	0.980-1.036
	0.978-1.022
	0.935-1.005

	p-value
	0.467
	0.381
	0.611
	0.99
	0.096

	LAG 1

	OR
	1.006
	1.029
	1.004
	1.002
	1.015

	95% CI
	0.852-1.189
	0.927-1.141
	0.973-1.037
	0.980-1.025
	0.976-1.057

	p-value
	0.941
	0.595
	0.786
	0.843
	0.448

	LAG 2

	OR
	1.008
	0.911
	0.988
	0.998
	0.997

	95% CI
	0.848-1.199
	0.818-1.014
	0.957-1.020
	0.975-1.021
	0.959-1.037

	p-value
	0.924
	0.089
	0.457
	0.84
	0.885

	LAG 3

	OR
	0.964
	1.038
	0.997
	1.008
	1.019

	95% CI
	0.812-1.145
	0.932-1.156
	0.966-1.030
	0.984-1.033
	0.979-1.061

	p-value
	0.677
	0.492
	0.867
	0.511
	0.351

	LAG 4

	OR
	0.943
	0.959
	0.989
	1.008
	0.972

	95% CI
	0.796-1.115
	0.863-1.066
	0.958-1.020
	0.985-1.031
	0.934-1.011

	p-value
	0.491
	0.438
	0.477
	0.506
	0.155

	LAG 5

	OR
	1.094
	1.066
	1.02
	0.988
	1.022

	95% CI
	0.925-1.294
	0.960-1.184
	0.989-1.053
	0.966-1.011
	0.983-1.063

	p-value
	0.293
	0.231
	0.21
	0.311
	0.279

	LAG 6

	OR
	1.053
	1.08
	1.009
	0.977
	0.979

	95% CI
	0.890-1.246
	0.965-1.187
	0.978-1.041
	0.951-1.003
	0.943-1.017

	p-value
	0.544
	0.2
	0.569
	0.077
	0.283

	LAG 7

	OR
	0.955
	0.962
	0.999
	1.020
	1.022

	95% CI
	0.825-1.106
	0.877-1.054
	0.971-1.027
	0.997-1.044
	0.987-1.058

	p-value
	0.541
	0.4
	0.934
	0.09
	0.216


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.


Table A11. Associations between the exposure to short-term pollutants and ischemic stroke incidence in the winter.
	Variables
	PM2.5
	PM10
	NO2
	SO2
	CO

	LAG 0

	OR
	1.109
	1.089
	1.028
	1.028
	2.303

	95% CI
	1.002-1.227
	1.010-1.174
	1.006-1.050
	0.980-1.079
	0.806-6.578

	p-value
	0.045
	0.026
	0.013
	0.26
	0.119

	LAG 1

	OR
	0.907
	0.916
	0.975
	1.007
	0.452

	95% CI
	0.807-1.021
	0.836-1.004
	0.951-1.000
	0.955-1.060
	0.126-1.616

	p-value
	0.105
	0.06
	0.047
	0.805
	0.222

	LAG 2

	OR
	1.019
	1.048
	1.012
	0.988
	1.118

	95% CI
	0.905-1.148
	0.957-1.148
	0.987-1.038
	0.935-1.043
	0.313-4.000

	p-value
	0.755
	0.309
	0.359
	0.662
	0.864

	LAG 3

	OR
	1.026
	0.983
	1.001
	1.028
	0.714

	95% CI
	0.906-1.163
	0.893-1.081
	0.976-1.027
	0.974-1.085
	0.187-2.724

	p-value
	0.681
	0.72
	0.925
	0.315
	0.622

	LAG 4

	OR
	1.059
	1.024
	1.016
	1.044
	1.807

	95% CI
	0.935-1.200
	0.931-1.127
	0.990-1.043
	0.991-1.101
	0.471-6.926

	p-value
	0.364
	0.625
	0.217
	0.106
	0.388

	LAG 5

	OR
	1.014
	1.052
	1.009
	0.979
	1.934

	95% CI
	0.900-1.142
	0.960-1.152
	0.983-1.036
	0.929-1.032
	0.524-7.141

	p-value
	0.824
	0.282
	0.492
	0.435
	0.322

	LAG 6

	OR
	0.921
	0.954
	0.99
	1.006
	0.404

	95% CI
	0.820-1.035
	0.872-1.043
	0.966-1.015
	0.954-1.061
	0.110-1.489

	p-value
	0.167
	0.3
	0.429
	0.817
	0.173

	LAG 7

	OR
	1.003
	0.986
	0.994
	1.012
	0.778

	95% CI
	0.910-1.105
	0.916-1.060
	0.972-1.016
	0.966-1.060
	0.266-2.274

	p-value
	0.96
	0.696
	0.59
	0.613
	0.646


Abbreviations: NO2, nitrogen dioxide; PM2.5, particulate matter with a diameter of 2.5 μm or less; PM10 particulate matter with a diameter of 10 μm or less; SO2, sulfur dioxide; CO, carbon monoxide; OR, odds ratio; 95% CI, 95% Confidence Intervals.





