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Figure S1. XRD patterns of iron hydroxide nanopetalines before and after As(III) and As(V) adsorption at pH 4.0 and 8.0.
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Figure S2. Full spectra of iron hydroxide nanopetalines before and after As(III) and As(V) adsorption at pH 4.0.
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