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Video 1: CNN-based CA measurements from a horizontal viewpoint. 
Video 2: CNN-based CA measurements from an angled viewpoint.
Video 3: SNR estimations based on pixel grayscale values.
Video 4: CNN-based CA measurement from double horizontal viewpoints.

