[bookmark: _Hlk148707860]Supporting Information: 
Dynamic Light Scattering for Particle Characterization Subjected to Ultrasound: A Study on Compact Particles and Acousto-responsive Microgels 
Sebastian Stock, Regine von Klitzing, and Amin Rahimzadeh*
[bookmark: _GoBack]Soft Matter at Interfaces, Institute for Condensed Matter Physics, Technische Universität Darmstadt, Hochschulstraße 8, 64289 Darmstadt, Germany
* Email address: Amin.rahimzadeh@pkm.tu-darmstadt.de 
[bookmark: _Hlk149208813][image: ]
Figure S1. NACF for pure water subjected to 255 kHz and 300 mV ultrasound and without US.  
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Figure S2. NACF of 200 nm Si particles subjected to the US in three different frequencies. 
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Figure S3. NACF of PNIPAM microgels cross-linked by 5 mol% BIS subjected to 5.4 MHz US immediately after starting and 300 s after starting actuation.
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