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Figure S1 XPS wide scan spectra of sample W and D; High-resolution XPS spectra of C 1s for sample W (b) and sample D (c). 
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Figure S2 High-resolution XPS spectra of Ti (a); Ag (b); and Si (c) for Sample D.
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