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Fig SI.1. Flowchart of the study on the treatment of clay with glass.
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Fig. SI.2 Proctor curves of studied mixtures
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Fig. SI.3 Evolution of compaction parameters as a function of glass content
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	Fig. SI.4 Influence of mixture addition on CBR curves after immersion
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