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	RC2000 Settings

	Application Width
	24 ft

	Machine Type
	Self Propelled Sprayer

	Application Mode
	Liquid Constant Flow

	Number of Sections
	12

	Section Valve Type
	3-wire

	Equal Width Sections
	yes

	Fence Rows Enabled
	no

	Section Width
	2 ft

	Pressure Sensor
	no

	Agitator Valve
	no

	Flow Return Installed
	no

	Control Valve Type
	none

	Flowmeter Calibration
	8000

	Flowmeter Pulse Units
	10 gal

	Tank Capacity
	0

	Current Level
	0

	Low Tank Level
	0

	Tank Fill Monitor
	0

	Preset Rate Value
	175

	Rate Bump
	0

	Rate Selection
	Map Based

	Rate Smoothing
	15%

	Decimal Shift
	1

	Off Rate Alarm
	30

	Alarm?
	no

	Minimum Flow Rate
	0



