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S.F.1. Sand granulation curve – comparison of the sand's particle size distribution with ASTM standard limits for concrete suitability
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S.F.2. Gravel granulation curve – comparison of the gravel's particle size distribution with ASTM standard limits, indicating compliance for suitability in concrete production
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