Supplementary Information
Supplemental Table S1 Spectral spread for the wavelengths of test flashes
	Wavelength (nm)
	Light source
	Bandpass filter
	Full width at half maximum (nm)

	405
	M405L4a
	(Not used)
	12.5

	425
	
	#87-787b
	

	450
	
	#88-300b
	

	475
	
	#87-788b
	

	500
	
	#88-300b
	

	525
	
	#87-789b
	

	550
	MNWHL4a
	#88-300b
	25

	575
	
	#87-790b
	

	600
	
	#88-300b
	

	625
	
	#87-791b
	

	650
	
	#88-300b
	

	675
	
	#87-792b
	

	aThorlabs, bEdmund Optics.
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Supplemental Figure S1 Waveform of rod-cone mixed responses after subtracting isolated cone component (Fig. 7c). Flash intensity: 32 to 32000 photons µm-2, Red: 320 photons µm-2. Timing of the test flash is shown by an arrow. Cone response-like bumps are still observed on the rod response plateau indicating incomplete rod-cone response separation.
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