Supplementary Table 1. Grand averaged peak latencies for each group, condition, and component.

	Analysis
	Component
	Condition
	Group
	Peak latency (ms)

	ERP
	P1
	Low Intensity
	Control
	70.3

	ERP
	P1
	Low Intensity
	Tinnitus
	62.5

	ERP
	P1
	High Intensity
	Control
	58.6

	ERP
	P1
	High Intensity
	Tinnitus
	58.6

	ERP
	P1
	Sub-tinnitus Frequency
	Control
	54.7

	ERP
	P1
	Sub-tinnitus Frequency
	Tinnitus
	58.5

	ERP
	P1
	Tinnitus Frequency
	Control
	58.6

	ERP
	P1
	Tinnitus Frequency
	Tinnitus
	58.6

	ERP
	N1
	Low Intensity
	Control
	128.9

	ERP
	N1
	Low Intensity
	Tinnitus
	121.1

	ERP
	N1
	High Intensity
	Control
	97.6

	ERP
	N1
	High Intensity
	Tinnitus
	97.7

	ERP
	N1
	Sub-tinnitus Frequency
	Control
	97.7

	ERP
	N1
	Sub-tinnitus Frequency
	Tinnitus
	89.8

	ERP
	N1
	Tinnitus Frequency
	Control
	101.6

	ERP
	N1
	Tinnitus Frequency
	Tinnitus
	89.8

	ERP
	P2
	Low Intensity
	Control
	203.1

	ERP
	P2
	Low Intensity
	Tinnitus
	175.8

	ERP
	P2
	High Intensity
	Control
	183.6

	ERP
	P2
	High Intensity
	Tinnitus
	195.3

	ERP
	P2
	Sub-tinnitus Frequency
	Control
	187.5

	ERP
	P2
	Sub-tinnitus Frequency
	Tinnitus
	214.8

	ERP
	P2
	Tinnitus Frequency
	Control
	207.0

	ERP
	P2
	Tinnitus Frequency
	Tinnitus
	152.3

	RP
	
	Low Intensity
	Control
	199.2

	RP
	
	Low Intensity
	Tinnitus
	121.1

	RP
	
	High Intensity
	Control
	125.0

	RP
	
	High Intensity
	Tinnitus
	136.7

	RP
	
	Sub-tinnitus Frequency
	Control
	117.2

	RP
	
	Sub-tinnitus Frequency
	Tinnitus
	113.3

	RP
	
	Tinnitus Frequency
	Control
	179.7

	RP
	
	Tinnitus Frequency
	Tinnitus
	164.1

	MMN
	
	Low Intensity
	Control
	249.8

	MMN
	
	Low Intensity
	Tinnitus
	171.9

	MMN
	
	High Intensity
	Control
	210.9

	MMN
	
	High Intensity
	Tinnitus
	152.3

	MMN
	
	Sub-tinnitus Frequency
	Control
	160.2

	MMN
	
	Sub-tinnitus Frequency
	Tinnitus
	175.8

	MMN
	
	Tinnitus Frequency
	Control
	199.2

	MMN
	
	Tinnitus Frequency
	Tinnitus
	132.8



Table 1. P1, N1 and P2 peaks were identified from ERP responses. RP peaks were identified from repetition positivity waveforms. MMN peaks were identified from deviant-minus-standard difference waveforms. Mean ERP amplitudes were calculated within ±10 ms windows centred on the listed group-level peak latencies.

