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Fig. S1.  TEM image of γ-alumina
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Fig. S2.  SEM image of Super Activated Carbon
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Fig. S3. Photograph of the laboratory apparatus employed in the experimental study of CO₂ absorption.
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	Fig. S4. Schematic diagram of adsorption set-up. 
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Fig. S5. CO2 adsorption curve at isotherm 313.15 K.
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Fig. S6. Langmuir isotherm (T=313.15 K).
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Fig. S7. Freundlich isotherm (T=313.15 K).
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