Additional file 1

Genetic diversity at 13 microsatellite loci for 12 sites of the Chinese wood frog (Rana chensinensis). N, sample size; A, number of alleles; Ar, allele richness; HO, observed heterozygosity; HE, expected heterozygosity; FIS value; PHW, exact P-value for Hardy-Weinberg equilibrium test.

	Sites
	
	RCM

S007
	RCM

S009
	RCM

S010
	RCM

S011
	RCM

S026
	RCM

S028
	RCM

S029
	RCM

S030
	RCM

S035
	RCM

S042
	RCM

S092
	RCM

S098
	RCM

S107
	Average

	1
	A/Ar
	16/14.3
	10/8.6
	9/8.5
	10/9.3
	10/9.5
	9/8.3
	8/7.3
	9/8.2
	13/11.9
	12/11.1
	9/8.4
	9/7.9
	15/12.8
	10.7/9.7

	N = 37
	HO
	0.833
	0.730
	0.706
	0.583
	0.946
	0.865
	0.676
	0.784
	0.838
	0.919
	0.838
	0.667
	0.784
	0.782

	
	HE
	0.891
	0.773
	0.837
	0.804
	0.853
	0.836
	0.723
	0.734
	0.895
	0.864
	0.840
	0.668
	0.837
	0.812

	
	FIS
	0.065
	0.056
	0.158
	0.277
	-0.111
	-0.036
	0.066
	-0.069
	0.063
	-0.064
	0.003
	0.002
	0.065
	0.036

	
	PHW
	0.035
	0.924
	0.159
	0.020
	0.000
	0.132
	0.174
	0.659
	0.091
	0.448
	0.586
	0.082
	0.276
	—

	2
	A/Ar
	17/17.0
	6/6.0
	11/10.9
	10/10.0
	10/10.0
	9/8.9
	7/7.0
	10/9.9
	11/10.8
	12/11.8
	6/6.0
	4/4.0
	9/9.0
	9.4/9.3

	N = 26
	HO
	0.840
	0.731
	0.692
	0.560
	0.962
	0.769
	0.769
	0.846
	0.808
	0.808
	0.769
	0.577
	0.923
	0.773

	
	HE
	0.936
	0.775
	0.783
	0.842
	0.873
	0.817
	0.752
	0.864
	0.861
	0.857
	0.693
	0.581
	0.837
	0.805

	
	FIS
	0.104
	0.058
	0.118
	0.34
	-0.104
	0.059
	-0.025
	0.02
	0.063
	0.058
	-0.112
	0.008
	-0.105
	0.037

	
	PHW
	0.139
	0.720
	0.036
	0.001
	0.111
	0.208
	0.554
	0.360
	0.213
	0.863
	0.105
	0.785
	0.516
	—

	3
	A/Ar
	16/13.2
	8/6.6
	8/6.5
	8/7.7
	8/6.7
	20/16.2
	14/11.3
	13/10.8
	20/15.8
	21/17.3
	12/10.0
	12/10.3
	14/11.7
	13.4/11.1

	N = 50
	HO
	0.420
	0.580
	0.240
	0.620
	0.780
	0.740
	0.600
	0.840
	0.900
	0.800
	0.700
	0.800
	0.620
	0.665

	
	HE
	0.912
	0.725
	0.822
	0.815
	0.806
	0.887
	0.820
	0.864
	0.908
	0.916
	0.857
	0.828
	0.806
	0.844

	
	FIS
	0.486
	0.202
	0.693
	0.241
	0.032
	0.167
	0.270
	0.028
	0.009
	0.128
	0.163
	0.034
	0.233
	0.207

	
	PHW
	0.000
	0.088
	0.000
	0.012
	0.452
	0.023
	0.002
	0.531
	0.094
	0.006
	0.301
	0.159
	0.000
	—

	4
	A/Ar
	20/14.9
	12/11.1
	11/9.6
	12/9.9
	9/8.0
	20/15.3
	21/17.0
	11/10.2
	15/12.3
	20/15.7
	12/10.7
	16/12.2
	14/12.0
	14.8/12.2

	N = 50
	HO
	0.620
	0.780
	0.240
	0.700
	0.680
	0.800
	0.340
	0.680
	0.660
	0.860
	0.620
	0.580
	0.740
	0.638

	
	HE
	0.868
	0.871
	0.861
	0.890
	0.834
	0.872
	0.882
	0.829
	0.877
	0.915
	0.862
	0.780
	0.777
	0.855

	
	FIS
	0.269
	0.106
	0.669
	0.195
	0.186
	0.083
	0.527
	0.181
	0.209
	0.038
	0.283
	0.259
	0.048
	0.235

	
	PHW
	0.000
	0.256
	0.000
	0.060
	0.135
	0.043
	0.000
	0.002
	0.004
	0.266
	0.000
	0.002
	0.226
	—


	Sites
	
	RCM

S007
	RCM

S009
	RCM

S010
	RCM

S011
	RCM

S026
	RCM

S028
	RCM

S029
	RCM

S030
	RCM

S035
	RCM

S042
	RCM

S092
	RCM

S098
	RCM

S107
	Average

	5
	A/Ar
	8/8.0
	7/6.7
	10/9.6
	8/7.8
	9/8.4
	7/6.7
	9/8.5
	8/7.6
	12/10.8
	8/8.0
	5/4.7
	11/10.6
	9/8.5
	8.5/8.2

	N = 35
	HO
	0.143
	0.706
	0.818
	0.333
	0.912
	0.735
	0.581
	0.824
	0.576
	0.879
	0.576
	0.879
	0.594
	0.658

	
	HE
	0.733
	0.750
	0.867
	0.806
	0.813
	0.741
	0.692
	0.773
	0.636
	0.858
	0.641
	0.851
	0.672
	0.756

	
	FIS
	0.808
	0.059
	0.057
	0.59
	-0.123
	0.008
	0.163
	-0.067
	0.096
	-0.025
	0.103
	-0.033
	0.118
	0.135

	
	PHW
	0.000
	0.177
	0.018
	0.000
	0.132
	0.427
	0.023
	0.309
	0.306
	0.419
	0.374
	0.904
	0.075
	—

	6
	A/Ar
	11/9.0
	10/9.1
	9/8.7
	9/8.1
	8/7.1
	15/12.0
	9/8.2
	9/8.7
	13/11.5
	13/12.7
	12/9.6
	9/8.0
	12/10.3
	10.7/9.5

	N = 48
	HO
	0.478
	0.739
	0.600
	0.546
	0.522
	0.717
	0.217
	0.761
	0.804
	0.841
	0.783
	0.750
	0.778
	0.657

	
	HE
	0.523
	0.728
	0.806
	0.828
	0.813
	0.726
	0.720
	0.835
	0.802
	0.914
	0.851
	0.699
	0.856
	0.777

	
	FIS
	0.087
	-0.016
	0.258
	0.344
	0.361
	0.012
	0.7
	0.089
	-0.003
	0.081
	0.081
	-0.074
	0.093
	0.155

	
	PHW
	0.220
	0.111
	0.193
	0.000
	0.000
	0.829
	0.000
	0.220
	0.045
	0.100
	0.542
	0.371
	0.367
	—

	7
	A/Ar
	4/3.8
	14/12.9
	8/7.9
	7/6.9
	7/6.5
	6/5.3
	8/7.7
	6/5.5
	8/6.6
	14/12.1
	9/8.2
	11/9.3
	9/6.4
	8.5/7.6

	N = 45
	HO
	0.311
	0.778
	0.535
	0.707
	0.727
	0.422
	0.257
	0.533
	0.533
	0.857
	0.844
	0.800
	0.578
	0.606

	
	HE
	0.408
	0.908
	0.858
	0.825
	0.783
	0.501
	0.821
	0.491
	0.617
	0.840
	0.790
	0.785
	0.631
	0.712

	
	FIS
	0.239
	0.145
	0.38
	0.144
	0.072
	0.159
	0.69
	-0.088
	0.137
	-0.02
	-0.07
	-0.019
	0.086
	0.143

	
	PHW
	0.030
	0.001
	0.000
	0.118
	0.560
	0.186
	0.000
	0.832
	0.174
	0.088
	0.101
	0.241
	0.506
	—

	8
	A/Ar
	10/7.6
	17/14.2
	12/9.6
	13/12.1
	8/7.4
	19/12.6
	19/15.6
	11/10.6
	19/15.6
	22/18.2
	11/10.2
	13/10.7
	13/11.2
	14.4/12.0

	N = 50
	HO
	0.200
	0.780
	0.500
	0.680
	0.800
	0.700
	0.400
	0.900
	0.800
	0.920
	0.940
	0.720
	0.780
	0.702

	
	HE
	0.693
	0.915
	0.864
	0.841
	0.806
	0.716
	0.913
	0.862
	0.918
	0.939
	0.835
	0.707
	0.855
	0.836

	
	FIS
	0.690
	0.149
	0.408
	0.193
	0.007
	0.022
	0.522
	-0.045
	0.130
	0.020
	-0.127
	-0.019
	0.088
	0.157

	
	PHW
	0.000
	0.002
	0.000
	0.070
	0.107
	0.275
	0.000
	0.307
	0.064
	0.133
	0.312
	0.830
	0.000
	—


	Sites
	
	RCM

S007
	RCM

S009
	RCM

S010
	RCM

S011
	RCM

S026
	RCM

S028
	RCM

S029
	RCM

S030
	RCM

S035
	RCM

S042
	RCM

S092
	RCM

S098
	RCM

S107
	Average

	9
	A/Ar
	8/5.9
	19/16.1
	12/9.7
	10/9.2
	9/7.0
	16/10.4
	13/10.6
	11/9.7
	18/14.2
	18/15.3
	12/11.1
	16/11.1
	11/9.7
	13.3/10.8

	N = 50
	HO
	0.220
	0.860
	0.700
	0.860
	0.780
	0.520
	0.280
	0.800
	0.720
	0.860
	0.900
	0.640
	0.660
	0.677

	
	HE
	0.644
	0.919
	0.847
	0.845
	0.794
	0.577
	0.824
	0.826
	0.868
	0.924
	0.887
	0.639
	0.815
	0.801

	
	FIS
	0.575
	0.065
	0.152
	-0.018
	-0.014
	0.099
	0.578
	0.032
	0.172
	0.026
	-0.014
	-0.047
	0.192
	0.138

	
	PHW
	0.000
	0.232
	0.099
	0.701
	0.871
	0.169
	0.000
	0.169
	0.000
	0.260
	0.523
	0.890
	0.028
	—

	10
	A/Ar
	5/4.8
	11/10.9
	5/4.7
	8/8.0
	8/7.6
	7/6.9
	9/8.5
	11/9.9
	9/8.3
	9/8.6
	10/8.9
	11/10.4
	9/8.7
	8.6/8.2

	N = 32
	HO
	0.500
	0.875
	0.531
	0.321
	0.813
	0.742
	0.129
	0.719
	0.563
	0.750
	0.813
	0.774
	0.400
	0.610

	
	HE
	0.560
	0.901
	0.572
	0.844
	0.801
	0.677
	0.766
	0.803
	0.771
	0.838
	0.783
	0.847
	0.819
	0.768

	
	FIS
	0.109
	0.03
	0.072
	0.623
	-0.015
	-0.098
	0.834
	0.106
	0.274
	0.107
	-0.038
	0.087
	0.516
	0.201

	
	PHW
	0.257
	0.039
	0.699
	0.000
	0.5215
	0.404
	0.000
	0.705
	0.407
	0.034
	0.396
	0.045
	0.000
	—

	11
	A/Ar
	3/2.8
	9/8.8
	8/7.3
	3/3.0
	3/2.9
	2/2.0
	2/1.8
	4/3.4
	5/4.3
	4/4.0
	4/3.9
	2/2.0
	8/7.2
	4.4/4.1

	N = 50
	HO
	0.200
	0.833
	0.489
	0.082
	0.939
	0.449
	0.000
	0.306
	0.580
	0.760
	0.306
	0.320
	0.457
	0.200

	
	HE
	0.185
	0.858
	0.826
	0.511
	0.542
	0.488
	0.040
	0.391
	0.584
	0.707
	0.339
	0.298
	0.779
	0.504

	
	FIS
	-0.082
	0.029
	0.410
	0.842
	-0.745
	0.081
	1.000
	0.219
	0.007
	-0.076
	0.098
	-0.074
	0.417
	0.164

	
	PHW
	1.000
	0.883
	0.000
	0.000
	0.000
	0.767
	0.010
	0.190
	0.473
	0.305
	0.056
	1.000
	0.000
	—

	12
	A/Ar
	2/2.0
	11/10.2
	9/7.8
	4/3.5
	3/3.0
	12/10.8
	10/8.8
	4/3.5
	11/10.7
	10/8.1
	6/5.9
	10/9.0
	7/5.3
	7.6/6.8

	N = 50
	HO
	0.333
	0.760
	0.447
	0.213
	0.872
	0.792
	0.08
	0.265
	0.222
	0.523
	0.857
	0.936
	0.604
	0.531

	
	HE
	0.281
	0.832
	0.693
	0.252
	0.616
	0.831
	0.714
	0.306
	0.855
	0.665
	0.796
	0.739
	0.618
	0.631

	
	FIS
	-0.19
	0.087
	0.358
	0.157
	-0.423
	0.047
	0.889
	0.133
	0.743
	0.216
	-0.077
	-0.273
	0.022
	0.130

	
	PHW
	0.323
	0.076
	0.000
	0.156
	0.000
	0.375
	0.792
	0.095
	0.000
	0.122
	0.183
	0.048
	0.828
	—


