Additional File 2. Phase II results.  Colorimetric water testing from phase I was discontinued because of a lack of consensus about results accuracy. Data show home 2010 with very high lead levels. Home 2030 data may suggest indoor sources of mold (indoor/outdoor >30). Other parameters do not indicate exposures of concern. 
	Home ID
	date tested
	time of day
	basement radon (pCi/L)
	mold indoors (total spores/m3)
	location
	mold outdoors (total spores/m3)
	location
	lead in wall paint (no.+ve/total no)
	location
	lead in floor dust1 (µg/ft2) - 1st
	location
	lead in floor dust1 (µg/ft2) - 2nd
	location
	lead in floor dust1 (µg/ft2) - 3rd
	location
	lead in sill dust2 (µg/ft2) - 1st
	location
	lead in sill dust2 (µg/ft2) - 2nd
	location
	lead in sill dust2 (µg/ft2) - 3rd
	location
	tap water 1st draw (ppb)
	tap water 2nd draw (ppb)
	PM2.5 living room – mean3 (µg/m3)
	PM2.5 kitchen – mean3 (µg/m3)

	2000
	2/01/08
	9:30
	2.3
	150
	KT
	170
	HW
	1/6
	LR
	<
	L R
	<
	BR
	<
	KT
	<
	LR
	<
	BR
	17
	KT
	36.7
	1.7
	9
	8

	2010
	2/01/08
	16:45
	0.6
	30
	HW
	30
	EN
	1/6
	BR
	<
	L R
	<
	BR
	<
	HW
	15000
	LR
	2100
	BR
	45.0
	DR
	1.1
	<1
	3
	4

	2020
	2/06/08
	18:50
	n/a
	120
	KT
	360
	EN
	0/6
	n/a
	<
	LR
	<
	BR
	<
	KT
	<
	LR
	<
	BR
	n/a
	n/a
	-
	-
	5
	6

	2030
	3/03/08
	10:30
	n/a
	1410
	LR
	36
	WW
	5/6
	*
	9.8
	LR
	<
	BR
	27.0
	KT
	19.0
	LR
	<
	BR
	13.0
	KT
	2.7
	1
	59
	72

	2040
	3/03/08
	14:50
	0.1
	350
	LR
	36
	WW
	1/6
	BR
	<
	LR
	<
	KT
	n/a
	n/a
	18.0
	LR
	21.0
	BA
	n/a
	n/a
	<1
	<1
	9
	9

	2050
	3/19/08
	15:30
	n/a
	30
	LR
	10
	PO
	1/6
	KT
	<
	DR
	<
	KT
	0*
	BR
	<
	DR
	<
	KT
	<
	BR
	15
	<1
	7
	7


1 lead-in-floor-dust USEPA standard ≤ 40 µg/ft2; 2 lead-in-sill-dust USEPA standard ≤ 250 µg/ft2; 3 30-minute mean.
Key: LR - living room, BR - bedroom, DR - dining room, KT - kitchen, w.sill - window sill, HW - hallway, EN - entrance, PO - porch, WW - walkway, BA – bathroom; *KT wall, office baseboard, BR mirror, BA wall, HW wall next to BR; < below detection limit; - resident did not take sample.






