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FigureS4. Dark current-voltage characteristic curves of CuInS2 based QDSSC with (red dots) and without (black squares) In2S3 buffer layer.
FigureS5. IPCE spectra of CuInS2 QD-sensitized solar cell with different SILAR cycles.

