Additional file 1 –Table S1.

Comparison of average rectal temperatures and clinical sign scores of with each group on days postinoculation.
	DPI
	Groups
	Average rectal temperature
	Significant difference level
	Groups
	Clinical sign score
	Significant difference level

	
	
	
	p<0.05
	p<0.01
	
	
	p<0.05
	p<0.01

	0
	HP-PRRSV
	39.3±0.15
	a
	A
	HP-PRRSV/PCV2
	0±0
	a
	A

	
	HP-PRRSV+PCV2
	39.2±0.11
	a
	A
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	HP-PRRSV/PCV2
	39.2±0.13
	a
	A
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.2±0.12
	a
	A
	HP-PRRSV
	0±0
	a
	A

	
	PCV2
	39.2±0.10
	a
	A
	PCV2
	0±0
	a
	A

	
	Control
	39.1±0.11
	a
	A
	Control
	0±0
	a
	A

	1
	HP-PRRSV/PCV2
	39.5±0.13
	a
	A
	HP-PRRSV/PCV2
	0±0
	a
	A

	
	HP-PRRSV+PCV2
	39.5±0.12
	ab
	A
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	HP-PRRSV
	39.2±0.32
	bc
	A
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	PCV2
	39.2±0.13
	c
	A
	HP-PRRSV
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.1±0.12
	c
	A
	PCV2
	0±0
	a
	A

	
	Control
	39.1±0.11
	c
	A
	Control
	0±0
	a
	A

	2
	HP-PRRSV/PCV2
	40.4±0.23
	a
	A
	HP-PRRSV/PCV2
	0.2±0.52
	a
	A

	
	HP-PRRSV+PCV2
	40.2±0.19
	ab
	AB
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	HP-PRRSV
	39.6±0.28
	abc
	ABC
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	PCV2
	39.4±0.10
	d
	C
	HP-PRRSV
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.3±0.13
	d
	C
	PCV2
	0±0
	a
	A

	
	Control
	39.1±0.14
	d
	C
	Control
	0±0
	a
	A

	3
	HP-PRRSV/PCV2
	39.9±0.15
	a
	A
	HP-PRRSV/PCV2
	0.4±0.43
	a
	A

	
	HP-PRRSV+PCV2
	39.8±0.12
	ab
	AB
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	HP-PRRSV
	39.7±0.15
	abc
	ABC
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	PCV2
	39.4±0.13
	d
	ABC
	HP-PRRSV
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.1±0.23
	d
	C
	PCV2
	0±0
	a
	A

	
	Control
	39.1±0.13
	d
	C
	Control
	0±0
	a
	A

	4
	HP-PRRSV+PCV2
	39.7±0.11
	a
	A
	HP-PRRSV/PCV2
	0±0
	a
	A

	
	HP-PRRSV/PCV2
	39.6±0.12
	ab
	A
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.5±0.14
	abc
	A
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	HP-PRRSV
	39.5±0.13
	abc
	A
	HP-PRRSV
	0±0
	a
	A

	
	PCV2
	39.4±0.11
	abc
	A
	PCV2
	0±0
	a
	A

	
	Control
	39.1±0.10
	c
	A
	Control
	0±0
	a
	A

	5
	HP-PRRSV+PCV2
	39.8±0.12
	a
	A
	HP-PRRSV/PCV2
	0.4±0.42
	a
	A

	
	HP-PRRSV/PCV2
	39.8±0.13
	ab
	AB
	HP-PRRSV
	0.3±0.51
	a
	A

	
	HP-PRRSV
	39.8±0.12
	abc
	ABC
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	PCV2/HP-PRRSV
	39.6±0.13
	abcd
	ABC
	HP-PRRSV+PCV2
	0±0
	a
	A

	
	PCV2
	39.5±0.11
	abcde
	ABC
	PCV2
	0±0
	a
	A

	
	Control
	39.2±0.14
	f
	C
	Control
	0±0
	a
	A

	6
	HP-PRRSV/PCV2
	40.4±0.15
	a
	A
	HP-PRRSV
	0.4±0.4
	a
	A

	
	HP-PRRSV+PCV2
	40.3±0.14
	ab
	AB
	HP-PRRSV/PCV2
	0.2±0.45
	a
	A

	
	HP-PRRSV
	40.1±0.15
	abc
	ABC
	HP-PRRSV+PCV2
	0.2±0.52
	a
	A

	
	PCV2/HP-PRRSV
	39.4±0.13
	d
	D
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	PCV2
	39.4±0.14
	d
	D
	PCV2
	0±0
	a
	A

	
	Control
	39.2±0.11
	d
	D
	Control
	0±0
	a
	A

	7
	HP-PRRSV/PCV2
	40.3±0.13
	a
	A
	HP-PRRSV
	1.8±0.54
	a
	A

	
	HP-PRRSV+PCV2
	40.1±0.12
	ab
	AB
	HP-PRRSV+PCV2
	1.4±0.48
	a
	A

	
	HP-PRRSV
	39.9±0.15
	abc
	ABC
	PCV2
	0.8±0.43
	a
	A

	
	PCV2/HP-PRRSV
	39.5±0.14
	d
	D
	HP-PRRSV/PCV2
	0.6±0.51
	a
	A

	
	PCV2
	39.4±0.12
	d
	D
	PCV2/HP-PRRSV
	0±0
	a
	A

	
	Control
	39.2±0.11
	d
	D
	Control
	0±0
	a
	A

	8
	HP-PRRSV/PCV2
	40.0±0.12
	a
	A
	HP-PRRSV+PCV2
	1.8±0.43
	a
	A

	
	HP-PRRSV+PCV2
	39.8±0.13
	ab
	AB
	HP-PRRSV
	1.8±0.41
	a
	A

	
	HP-PRRSV
	39.7±0.14
	abc
	AB
	HP-PRRSV/PCV2
	1.4±0.40
	a
	A

	
	PCV2/HP-PRRSV
	39.5±0.13
	d
	B
	PCV2
	1.2±0.51
	a
	A

	
	PCV2
	39.4±0.13
	de
	B
	PCV2/HP-PRRSV
	0±0
	b
	B

	
	Control
	39.1±0.11
	f
	B
	Control
	0±0
	b
	B

	9
	HP-PRRSV+PCV2
	40.5±0.13
	a
	A
	HP-PRRSV
	2.6±0.46
	a
	A

	
	HP-PRRSV/PCV2
	40.3±0.12
	ab
	AB
	HP-PRRSV+PCV2
	2.6±0.45
	ab
	A

	
	HP-PRRSV
	40.1±0.14
	abc
	ABC
	HP-PRRSV/PCV2
	1.6±0.42
	abc
	A

	
	PCV2/HP-PRRSV
	39.8±0.12
	d
	CD
	PCV2
	1.2±0.52
	cd
	A

	
	PCV2
	39.5±0.11
	e
	D
	PCV2/HP-PRRSV
	0.6±0.53
	cde
	A

	
	Control
	39.3±0.11
	e
	D
	Control
	0±0
	f
	B

	10
	HP-PRRSV+PCV2
	40.6±0.12
	a
	A
	HP-PRRSV+PCV2
	3±0.45
	a
	A

	
	HP-PRRSV/PCV2
	40.5±0.11
	ab
	AB
	HP-PRRSV
	2.8±0.56
	ab
	A

	
	PCV2/HP-PRRSV
	40.3±0.14
	abc
	ABC
	HP-PRRSV/PCV2
	2±0.43
	abc
	A

	
	HP-PRRSV
	40.0±0.13
	bcd
	ABCD
	PCV2
	1.6±0.56
	abcd
	A

	
	PCV2
	39.5±0.12
	e
	E
	PCV2/HP-PRRSV
	1±0.54
	e
	A

	
	Control
	39.2±0.10
	f
	E
	Control
	0±0
	f
	B

	11
	HP-PRRSV/PCV2
	40.6±0.14
	a
	A
	HP-PRRSV+PCV2
	3.6±0.62
	a
	A

	
	HP-PRRSV+PCV2
	40.4±0.14
	ab
	AB
	HP-PRRSV
	2.8±0.61
	ab
	A

	
	HP-PRRSV
	40.2±0.13
	bc
	ABC
	HP-PRRSV/PCV2
	2.2±0.51
	abc
	A

	
	PCV2/HP-PRRSV
	40.0±0.12
	bcd
	ABCD
	PCV2
	1.4±0.43
	abcd
	A

	
	PCV2
	39.6±0.10
	e
	E
	PCV2/HP-PRRSV
	0.6±0.52
	e
	A

	
	Control
	39.2±0.10
	f
	E
	Control
	0±0
	f
	B

	12
	HP-PRRSV+PCV2
	40.4±0.14
	a
	A
	HP-PRRSV+PCV2
	4±0.46
	a
	A

	
	HP-PRRSV/PCV2
	40.3±0.11
	ab
	AB
	HP-PRRSV/PCV2
	2.8±0.54
	b
	AB

	
	PCV2/HP-PRRSV
	40.2±0.13
	abc
	ABC
	HP-PRRSV
	2.6±0.54
	bc
	ABC

	
	HP-PRRSV
	40.1±0.14
	abcd
	ABCD
	PCV2
	1.4±0.46
	d
	BCD

	
	PCV2
	39.8±0.11
	e
	E
	PCV2/HP-PRRSV
	0.6±0.52
	de
	BCDE

	
	Control
	39.3±0.12
	f
	F
	Control
	0±0
	f
	F

	13
	PCV2/HP-PRRSV
	40.5±0.14
	a
	A
	HP-PRRSV+PCV2
	4.2±0.54
	a
	A

	
	HP-PRRSV/PCV2
	40.3±0.13
	ab
	AB
	HP-PRRSV/PCV2
	2.8±0.46
	b
	AB

	
	HP-PRRSV
	40.1±0.15
	abc
	ABC
	HP-PRRSV
	2±0.45
	bc
	ABC

	
	HP-PRRSV+PCV2
	39.8±0.16
	cd
	CD
	PCV2
	1.4±0.53
	bcd
	BCD

	
	PCV2
	39.7±0.13
	de
	DE
	PCV2/HP-PRRSV
	0.8±0.52
	de
	BCDE

	
	Control
	39.1±0.12
	f
	F
	Control
	0±0
	f
	F

	14
	PCV2/HP-PRRSV
	40.3±0.13
	a
	A
	HP-PRRSV+PCV2
	6.2±0.56
	a
	A

	
	HP-PRRSV/PCV2
	40.3±0.12
	ab
	AB
	HP-PRRSV/PCV2
	3.2±0.53
	b
	B

	
	HP-PRRSV
	40.3±0.11
	abc
	ABC
	HP-PRRSV
	3±0.46
	bc
	BC

	
	HP-PRRSV+PCV2
	39.9±0.12
	abcd
	ABCD
	PCV2/HP-PRRSV
	1.8±0.52
	d
	BCD

	
	PCV2
	39.5±0.11
	de
	DE
	PCV2
	1.6±0.53
	de
	BCDE

	
	Control
	39.2±0.13
	f
	E
	Control
	0±0
	f
	F

	15
	PCV2/HP-PRRSV
	40.2±0.14
	a
	A
	HP-PRRSV+PCV2
	6±0.41
	a
	A

	
	HP-PRRSV
	40.2±0.15
	ab
	AB
	HP-PRRSV/PCV2
	5±0.46
	ab
	AB

	
	HP-PRRSV/PCV2
	40.1±0.14
	abc
	ABC
	HP-PRRSV
	4.6±0.52
	abc
	ABC

	
	HP-PRRSV+PCV2
	39.8±0.13
	d
	ABCD
	PCV2/HP-PRRSV
	1.8±0.52
	d
	D

	
	PCV2
	39.6±0.13
	de
	DE
	PCV2
	1.6±0.54
	de
	DE

	
	Control
	39.3±0.11
	f
	E
	Control
	0±0
	f
	F

	16
	PCV2/HP-PRRSV
	40.2±0.13
	a
	A
	HP-PRRSV/PCV2
	5.4±0.43
	a
	A

	
	HP-PRRSV/PCV2
	40.1±0.13
	ab
	AB
	HP-PRRSV+PCV2
	5.2±0.48
	ab
	AB

	
	HP-PRRSV
	40.1±0.12
	abc
	ABC
	HP-PRRSV
	3.8±0.50
	c
	ABC

	
	PCV2
	39.6±0.12
	d
	D
	PCV2/HP-PRRSV
	3.2±0.41
	cd
	CD

	
	HP-PRRSV+PCV2
	39.6±0.13
	de
	DE
	PCV2
	1.6±0.53
	e
	CDE

	
	Control
	39.2±0.10
	f
	F
	Control
	0±0
	f
	F

	17
	PCV2/HP-PRRSV
	40.3±0.13
	a
	A
	HP-PRRSV/PCV2
	5.8±0.53
	a
	A

	
	HP-PRRSV/PCV2
	40.1±0.13
	ab
	AB
	HP-PRRSV
	4.6±0.51
	b
	AB

	
	HP-PRRSV
	40.1±0.14
	abc
	ABC
	HP-PRRSV+PCV2
	4.4±0.32
	bc
	ABC

	
	PCV2
	39.5±0.12
	d
	D
	PCV2/HP-PRRSV
	3.2±0.56
	d
	CD

	
	HP-PRRSV+PCV2
	39.4±0.11
	de
	D
	PCV2
	1.4±0.52
	e
	E

	
	Control
	39.2±0.12
	f
	D
	Control
	0±0
	f
	F

	18
	HP-PRRSV/PCV2
	40.6±0.14
	a
	A
	HP-PRRSV/PCV2
	6.2±0.53
	a
	A

	
	PCV2/HP-PRRSV
	40.1±0.11
	b
	B
	HP-PRRSV+PCV2
	4.2±0.46
	b
	B

	
	HP-PRRSV
	39.7±0.13
	c
	C
	PCV2/HP-PRRSV
	4±0.46
	bc
	BC

	
	PCV2
	39.3±0.12
	d
	D
	HP-PRRSV
	3.8±0.54
	bcd
	BCD

	
	HP-PRRSV+PCV2
	39.3±0.14
	d
	D
	PCV2
	1.4±0.53
	e
	E

	
	Control
	39.1±0.11
	d
	D
	Control
	0±0
	f
	F

	19
	HP-PRRSV/PCV2
	40.3±0.14
	a
	A
	HP-PRRSV/PCV2
	5±0.50
	a
	A

	
	PCV2/HP-PRRSV
	40.1±0.13
	ab
	AB
	HP-PRRSV
	4±0.48
	b
	AB

	
	HP-PRRSV
	39.4±0.12
	c
	C
	PCV2/HP-PRRSV
	3.8±0.45
	bc
	ABC

	
	PCV2
	39.3±0.12
	cd
	C
	HP-PRRSV+PCV2
	3.8±0.46
	bcd
	ABCD

	
	Control
	39.2±0.12
	cd
	C
	PCV2
	1.4±0.43
	e
	E

	
	HP-PRRSV+PCV2
	39.0±0.15
	d
	C
	Control
	0±0
	f
	F

	20
	HP-PRRSV/PCV2
	40.3±0.13
	a
	A
	HP-PRRSV/PCV2
	5.8±0.43
	a
	A

	
	PCV2/HP-PRRSV
	40.0±0.12
	b
	AB
	PCV2/HP-PRRSV
	4.4±0.46
	b
	AB

	
	HP-PRRSV
	39.6±0.13
	c
	C
	HP-PRRSV
	4.2±0.47
	bc
	ABC

	
	HP-PRRSV+PCV2
	39.4±0.14
	cd
	C
	HP-PRRSV+PCV2
	3.8±0.52
	bcd
	ABCD

	
	PCV2
	39.3±0.14
	cde
	C
	PCV2
	1±0.57
	e
	E

	
	Control
	38.9±0.11
	f
	C
	Control
	0±0
	f
	F

	21
	HP-PRRSV/PCV2
	40.8±0.12
	a
	A
	HP-PRRSV/PCV2
	6.8±0.51
	a
	A

	
	PCV2/HP-PRRSV
	40.1±0.13
	b
	B
	PCV2/HP-PRRSV
	5±0.46
	b
	B

	
	HP-PRRSV
	39.6±0.12
	c
	C
	HP-PRRSV
	4.6±0.52
	bc
	BC

	
	HP-PRRSV+PCV2
	39.5±0.13
	cd
	CD
	HP-PRRSV+PCV2
	3.8±0.51
	bcd
	BCD

	
	PCV2
	39.2±0.12
	e
	E
	PCV2
	1±0.53
	e
	E

	
	Control
	39.1±0.10
	e
	E
	Control
	0±0
	f
	F


