Anaerobic Degradation under Sewage Plant Simulation Conditions (AnBUSDiC test)

Annex 2
Pictures
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Picture 1: Eudiometer
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Picture 2: Thermoblock used to keep test vessel temperature constant
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Picture 3: Detail of eudiometer – seal between test vessel and head unit
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Picture 4: Detail of eudiometer – seal of pressure release valve at top of head unit

[image: image5.jpg]



Picture 5: Meniscus of stop fluid in the eudiometer head unit and meniscus of stop fluid in the reservoir bottle should be at the same height throughout the test to avoid over- or under-pressure in the eudiometer.
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