


Figure 5: Expected number of failed machines (ENF and ENN) by varying  and  on the base for different parameters values of F and N.
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