Additional file 1
This is the typical EVLW algorithm published for the PiCCO™ system (11).
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Substitute GEDV with formula (2): 
[image: ]									(2)
and regroup: 
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According to formula (2):
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which is equivalent to the EVLW algorithm used by for the EV1000™ system:
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EVLWpicco = CO - Mtt — 1.25 - GEDVpicco
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GEDVpicco = CO - (Mtt — Dst)
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EVIWpicco = CO - Mtt — 1.25 - CO - (Mtt — Dst) = CO - Dst — 0.25 - CO - (Mtt — Dst)
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EVILWpicco = CO - Dst — 0.25 - GEDVpicco
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EVILWpicco = CO - Dst — (0.25 - GEDVpiceo)

EVLWyoumeview = CO - Dst — (0-25 : GEDVVDl'llITlEViEW)




