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	Patient number
	Mode of 
CRRTa
	Dialysate rate (ml/h)
	Filtration rate (ml/h)
	Blood flow (ml/min)
	Fluid removal (ml/h)
	Durationb of CRRT use (h)

	9
	CVVHDc
	2000
	-
	100-120
	50-100
	76

	17
	CVVHDFd
	1500
	1500
	100-130
	0-200
	48 

	22
	CVVHD
	2000
	-
	80-120
	100-200
	78 

	24
	CVVHD
	1000-2000
	-
	150
	80
	96 

	27
	CVVHDF
	1200
	1000-2000
	150
	50-250
	85 


a, continuous renal replacement therapy; b, within the 4 days of the study; c, continuous venovenous hemodialysis, used with Ultraflux® AV-1000S-filters (Fresenius, Bad Homburg, Germany); d, continuous venovenous hemodiafiltration, used with Ultraflux® AV-600S-filters (Fresenius).

