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Fig. S1 Adsorption removal efficiency of MB on Fe3O4 and Fe3O4/PCC MNPs, inset is the adsorption capacity of MB ([Fe3O4/PCC] = 1.0 g L-1, [Fe3O4] = 1.0 g L-1, [MB] = 0.1 mM, pH = 6.0, T = 30 °C)
