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[image: ]Figure A0 Location of photos in supplementary Material


Figure A1 Peak discharge is marked with red lines. The slide on the right and the street on the left.
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Figure A2: Overview of the complete slide with active area (red) and currently inactive area (light blue)
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[image: ]Figure A3: The workflow followed from UAV imagery to point Density Clouds.

[image: ]Figure A4: Images from the frontal slope area showing differences in vegetation December 2021 and May 2022.




















Figure A5: Additional ERT Profiles showing the subsurface horizontally (P3, P5, P6) and longitudinally (P4)
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Figure A6: Overview of sliding area towards the west. Retaining wall for a smaller landslide (see Figure 2). 
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Figure A7: Cracks in the trail that appeared during the flood, view towards the slide. 
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Figure A8: Position of Müsch landslide along the Ahr river, 
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