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	Equipment
	Hewlett-Packard 6890, 5973N Mass Selective Detector

	Column
	HP-1 capillary column (30m×0.25mm i.d. 0.25µm film thickness) (J & W Scientific Co., Folsom, CA, USA)

	Carrier gas
	He (60 ml/min.); head pressure of 30 kPa

	Source temp.
	230°C

	Oven conditions
	70°C (2min.) → 20°C/min. → 280°C (5min) 

	Injector temp.
	200°C

	Ionizing voltage
	70 ev



