Supplementary Table S1. The criteria for diagnosing aortic stenosis

	AS type
	Criteria

	High-gradient AS
	mean gradient ≥40 mmHg, Vmax ≥4.0 m/s, AVA ≤1 cm2 (or ≤0.6 cm2/m2)

	Low-flow, low-gradient AS with reduced LVEF 
	mean gradient <40 mmHg, AVA ≤1 cm2, SVi ≤35 mL/m2, 
LVEF <50%

	Low-flow, low-gradient AS with preserved LVEF
	mean gradient <40 mmHg, AVA ≤1 cm2, SVi ≤35 mL/m2, 
LVEF ≥50%

	Normal-flow, low-gradient AS with preserved EF
	mean gradient <40 mmHg, AVA ≤1 cm2, SVi >35 mL/m2, 
LVEF ≥50%

	Discordant high-gradient AS 
	mean gradient ≥40 mmHg, AVA >1 cm2



AS: aortic stenosis; AVA: aortic valve area; LVEF: left ventricular ejection fraction; Svi: stroke volume indexed for BSA, Vmax: Peak transvalvular velocity

