
Supplementary Table 1 The scanning parameters
	Sequence
	TR
	TE
	Matrix
	Field of view
	Slice thickness
	Slice gap

	T2WI
	2800 ms
	85 ms
	 256 × 192
	240 mm × 240 mm
	3mm
	1mm

	ceT1WI
	580 ms
	15 ms
	 256 × 192
	240 mm × 240 mm
	3mm
	1mm


ceT1WI, contrast-enhanced T1-weighted imaging; T2WI, T2-weighted imaging; TE Echo time; TR Repetition time.


















 Supplementary Table 2 The radiomics features selected from each sequence alone
	Sequence
	Image type
	Feature class
	Feature name

	T2WI
	Original
	Histogram
	Kurtosis

	
	WaveletHH
	Histogram
	Skewness

	
	WaveletLH
	GLCM
	Correlation

	
	LoG5mm
	GLRLM
	ShortRunHighGrayLevelEmphasis

	
	LoG3mm
	NGTDM
	Busyness

	
	WaveletHL
	GLCM
	JointEntropy

	ceT1WI
	Original
	GLSZM
	LargeAreaHighGrayLevelEmphasis

	
	LoG3mm
	Histogram
	Kurtosis

	
	WaveletHL
	Histogram
	Minimum

	
	Original
	GLCM
	ClusterShade

	
	WaveletHH
	Histogram
	Skewness

	　
	WaveletHL
	GLCM
	JointEntropy


GLCM, gray-level cooccurrence matrix; GLRLM gray-level run-length matrix; GLSZM gray-level size zone matrix; NGTDM neighboring gray tone difference matrix.
