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	Quality Control Parameter
	Average for the Panel

	Read counts
	9.7± 5.6 Mio

	Depth
	456.0± 197.3

	20x Coverage percentage
	97.8± 0.3%

	Insert size
	178.4± 8.4

	On target reads percentage
	68.26± 4.4

	Q30 base percentage 
	95.13± 1.7



