
Additional file 2. Twelve-month defocus area-under-the-curve and contrast-sensitivity outcomes
	Variable
	Trinova (n=170)
	Omni (n=170)
	Unadjusted P value
	BH-FDR P value

	Defocus AUC, distance range (0 to -0.50 D)
	0.018 ± 0.015
	0.028 ± 0.017
	<.001
	NA

	Defocus AUC, intermediate range (-1.00 to -2.00 D)
	0.080 ± 0.031
	0.124 ± 0.039
	<.001
	NA

	Defocus AUC, near range (-2.50 to -3.50 D)
	0.131 ± 0.032
	0.191 ± 0.048
	<.001
	NA

	Photopic contrast sensitivity, 3 cpd
	1.71 ± 0.09
	1.64 ± 0.10
	<.001
	<.001

	Photopic contrast sensitivity, 6 cpd
	1.54 ± 0.10
	1.48 ± 0.12
	<.001
	<.001

	Photopic contrast sensitivity, 12 cpd
	1.26 ± 0.10
	1.18 ± 0.10
	<.001
	<.001

	Photopic contrast sensitivity, 18 cpd
	0.98 ± 0.11
	0.96 ± 0.12
	.21
	.212

	Mesopic glare contrast sensitivity, 3 cpd
	1.38 ± 0.12
	1.33 ± 0.13
	<.001
	<.001

	Mesopic glare contrast sensitivity, 6 cpd
	1.12 ± 0.13
	1.07 ± 0.14
	<.001
	<.001

	Mesopic glare contrast sensitivity, 12 cpd
	0.88 ± 0.12
	0.84 ± 0.12
	.007
	.008

	Mesopic glare contrast sensitivity, 18 cpd
	0.70 ± 0.12
	0.65 ± 0.14
	.001
	.001


Note: Continuous variables are mean ± SD. Lower defocus AUC values indicate better overall logMAR performance across the specified defocus range. cpd = cycles per degree.
Note: Unadjusted P values are exploratory secondary comparisons. Benjamini-Hochberg false-discovery-rate (BH-FDR) adjustment was applied as a sensitivity analysis across the eight 12-month contrast-sensitivity comparisons only; defocus AUC rows were not included in this adjustment (NA). Seven of eight contrast-sensitivity comparisons remained significant after BH-FDR adjustment. cpd = cycles per degree; AUC = area under the curve.
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