Table 1: Reliability of 300-meter segments with segments over 300 meters.
	
	300-meter with over 300 meter segments
	

	Item 
	Percent agreement
	Kappa or ICC
	

	Pedestrian Infrastructure
	
	

	Presence of Sidewalks
	100
	1.00
	

	Sidewalk Continuity 
	100
	1.00
	

	Sidewalk Buffer 
	100
	1.00
	

	Sidewalk Quality 
	96.9
	0.89
	

	Pedestrian Sign/Timer
	100
	1.00
	

	Pedestrian Crossing Sign
	100
	1.00
	

	Crosswalk Markings 
	100
	1.00
	

	Benches
	96.9
	0.89
	

	Streetlights
	96.9
	0.96
	

	Curb Cuts 
	100
	1.00
	

	Curb Cut Quality
	100
	1.00
	

	Tactile Paving
	100
	1.00
	

	Traffic Calming and Streets
	
	
	

	Traffic Lights
	100
	1.00
	

	Traffic Island
	100
	1.00
	

	Stop Lines
	100
	1.00
	

	Stops Signs
	100
	1.00
	

	Curb Extension
	100
	N/A
	

	Speed Bump
	100
	1.00
	

	Bollards 
	100
	N/A
	

	Number of Traffic Lanes
	100
	1.00
	

	Number of Parking Lanes
	100
	1.00
	

	Driveways
	87.5
	0.75
	

	Building Characteristics 
	
	
	

	Building Height
	93.8
	0.85
	

	Building Setback 
	90.6
	0.80
	

	Building Design Variation
	90.6
	0.803
	

	Transit
	
	
	

	Presence of Transit
	100
	1.00
	

	Type of Transit 
	100
	1.00
	

	Transit Facilities
	96.9
	0.90
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	Bike Lanes 
	96.9
	0.87
	

	Bike Buffer
	96.9
	0.65
	

	Bike Facilities 
	100
	1.00
	

	Aesthetics 
	
	
	

	Presence of Trees
	84.4
	0.71
	

	Shade
	96.9
	0.94
	

	Nature Areas 
	100
	1.00
	

	Landscaping
	96.9
	0.93
	

	Landscape Maintenance
	96.9
	0.93
	

	Presence of Litter
	100
	1.00
	

	Graffiti
	100
	1.00
	

	Broken/Boarded Windows
	100
	1.00
	

	Attractive Segment
	96.9
	0.96
	




