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	TOTAL*
	Accessible toilets**
	Functional toilets***
	Private toilets****
	High quality toilets*****
	Usable******

	 
	
	Baseline
	Follow-up
	Baseline
	Follow-up
	Baseline
	Follow-up
	Baseline
	Follow-up
	Baseline
	Follow-up
	Baseline
	Follow-up

	All toilets

	Control
	131
	132
	110/131
	109/132
	104/110
	96/109
	56/104
	51/95
	72/104
	61/96
	39/131
	32/132

	
	
	
	84%
	83%
	95%
	88%
	54%
	54%
	69%
	64%
	30%
	24%

	Intervention
	124
	124
	105/124
	95/124
	95/105
	85/95
	51/96
	37/85
	65/95
	62/85
	36/124
	31/124

	
	
	
	85%
	77%
	90%
	89%
	53%
	44%
	68%
	73%
	29%
	25%

	 
	
	 
	 
	RR: 0.927
(CI: 0.627 – 1.160)
p = 0.737
	RR: 0.942 
(CI: 0.845 – 1.048)
p = 0.271
	RR: 0.779
(CI: 0.496 – 1.224)
p = 0.280
	RR: 1.07
(CI: 0.789 – 1.451)
p = 0.660
	RR: 0.856
(CI: 0.449 – 1.632)
p = 0.637

	All classroom toilets

	Control
	63
	67
	58/63
	57/67
	58/58
	57/57
	29/58
	31/57
	46/58
	38/57
	23/63
	20/67

	
	
	
	92%
	85%
	100%
	100%
	50%
	54%
	79%
	67%
	37%
	30%

	Intervention
	46
	50
	46/46
	46/50
	46/46
	46/46
	15/46
	15/46
	37/46
	28/46
	13/46
	10/50

	
	
	
	100%
	92%
	100%
	100%
	33%
	33%
	80%
	61%
	28%
	20%

	 
	
	 
	 
	RR: 1.005
(CI: 0.584 – 1.727)
p = 0.987
	Correlation >1
	RR: 0.669
(CI: 0.396 – 1.132)
p = 0.134
	RR:0.784
(CI: 0.553 – 1.092)
p=0.147
	RR: 0.581
(CI: 0.264 – 1.275)
p = 0.175

	Non-classroom toilets

	Control
	68
	65
	52/68
	52/65
	46/52
	39/52
	27/46
	20/39
	26/46
	23/39
	16/68
	12/65

	
	
	
	76%
	80%
	88%
	75%
	59%
	51%
	57%
	59%
	24%
	18%

	Intervention
	78
	74
	59/78
	49/74
	49/59
	39/49
	36/49
	22/39
	28/49
	34/39
	23/78
	21/74

	
	
	
	76%
	66%
	83%
	80%
	73%
	56%
	57%
	87%
	29%
	28%

	 
	
	 
	 
	RR: 0.881
(CI: 0.552 – 1.112)
p= 0.627
	RR: 0.897
(CI: 0.484 – 1.664)
p = 0.732
	RR: 0.971
(CI: 0.508 – 1.852)
p = 0.928
	RR: 1.483
(CI: 0.349 – 0.901)
p = 0.118
	RR: 1.313
(CI: 0.556 – 3.199)
p = 0.535



1. Toilets assigned for demolition excluded from analysis
2. Accessibility defined as door is not locked
3. Functional defined as water is available for flushing in either cubicle or block
4. Privacy defined as: no large gaps /hole in structure, toilet has a door, which closes completely, and locks from the inside. Toilets intended for pre-primary children can be classified as private without a lock on the inside. 
5. High quality toilets defined as those which scored more than 8.5/ 10 across a range of quality indicators.
6. Usable defined as Accessible, Functional, Private and Clean
