Table S2. TWA* recommendations from the European Commission of Employment, Social Affairs and Inclusion’s Scientific Committee on Occupational Exposure Limits (SCOEL) 

	Pollutant
	Respirable fraction (<10 microns ) 

	Mn
	0.05 mg/m3

	Ni
	0.01 mg Ni/m3

	Cr

	2.0 mg/m3 total dust (calculated as Cr)



*The time-weighted average (TWA) exposure limit - the maximum average concentration of a chemical in air for a normal 8-hour working day and 40-hour week
