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Supplement figure 1.The measurement of cage position. The cage position is calculated as a/b*100%. a, the distance between the anterior metal marker and the leading edge of the caudal endplate. b, the length of caudal endplate
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