The video here shows the ultrasound-guided procedure. First, the maximum angulation of fracture was located under ultrasound guidance. Second, a K-wire was inserted carefully advanced to the fracture gap. Third, the fracture was reduced by leveraging the K-wire. Finally, the reduction was assessed by ultrasound. arrow: the K-wire; asterisk, epiphyseal core of ossification of the radial head..

