Supplementary Data
Supplementary Table 1 Comparison of surface roughness between baseline and chewing cycles at 120,000, 240,000, and 360,000.
	Materials
	p-value*

	
	Baseline VS 120,000 Cycles
	Baseline VS 240,000 Cycles
	Baseline VS 360,000 Cycles

	CP
	<0.001
	<0.001
	0.008

	TW
	<0.001
	<0.001
	<0.001

	TN
	<0.001
	<0.001
	<0.001

	DIF
	<0.001
	<0.001
	<0.001

	FC
	0.003
	<0.001
	<0.001



* Analysed by one-way repeated ANOVA with LSD post–hoc analysis.
