Graph 1. Film thickness values (µm) obtained from single and double-layer applications of Clearfil Tri-S Bond and G2-Bond Universal systems.
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Graph 2. Immediate and after thermalcycles mean microtensile bond strength (µTBS) values and standard deviations for single and double-layer applications of Clearfil Tri-S Bond Universal and G2-Bond Universal.
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