1. Supplementary table
Supplementary Table S1. Mesh-convergence analysis based on the maximum implant von Mises stress calculated in Model 1 under Loading Scenario 1 (Force 1)
	Nominal element size (mm)
	Maximum implant von Mises stress (MPa)
	Relative change (%)
	Convergence assessment

	0.4
	22.135
	—
	Reference mesh

	0.3
	24.701
	10.39
	Above criterion

	0.2
	26.357
	6.28
	Above criterion

	0.1
	26.983
	2.32
	Acceptable (<3%)


Relative change (%) = |σᵢ − σᵢ₋₁| / |σᵢ| × 100, where σᵢ is the result from the finer mesh and σᵢ₋₁ is the result from the preceding coarser mesh.

