
Supplementary Table 1. Intraobserver and interobserver reproducibility of the final selected radiomic features
	Radiomic feature
	Filter
	Class 
	Intraobserver ICC
(95% CI)
	Interobserver ICC
(95% CI)

	Run Length Non-Uniformity
	Original
	Gray Level Run Length Matrix 
	0.91 (0.83–0.96)
	0.88 (0.77–0.94)

	Interquartile Range
	Wavelet-LLL
	First-Order 
	0.94 (0.88–0.97)
	0.90 (0.81–0.95)

	Dependence Non-Uniformity
	Wavelet-LLH
	Gray Level Dependence Matrix 
	0.89 (0.79–0.94)
	0.86 (0.74–0.93)

	Gray Level Non-Uniformity
	Wavelet-LLH
	Gray Level Dependence Matrix 
	0.92 (0.85–0.96)
	0.87 (0.76–0.93)

	Maximum
	Wavelet-LHL
	First-Order 
	0.96 (0.91–0.98)
	0.93 (0.86–0.97)

	Zone Variance
	Wavelet-LHH
	Gray Level Size Zone Matrix 
	0.88 (0.77–0.94)
	0.82 (0.67–0.91)

	Gray Level Non-Uniformity
	Wavelet-HLL
	Gray Level Dependence Matrix 
	0.90 (0.81–0.95)
	0.85 (0.72–0.92)

	Large Area Emphasis
	Wavelet-HLH
	Gray Level Size Zone Matrix 
	0.87 (0.75–0.93)
	0.80 (0.63–0.89)


ICC: Intraclass correlation coefficient, CI: Confidence interval, H: High-pass filter, L: Low-pass filter 

