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	Setting
	Value

	Volume
	40 µL

	Pipetting tool
	TS_300

	Transfer type
	Pipette

	Use filter tips
	True

	Change tips
	Before each aspiration

	Aspiration
	Default

	Dispensing
	Dispense from defined height: 10.0 mm from bottom. No additional movement.

	Mix before aspirating
	False

	Mix after dispensing
	False

	Standard liquid type
	Protein

	Change parameter
	Yes (modified)

	Aspiration speed
	7 mm/s

	Dispensing speed
	7 mm/s

	Blow delay
	0 ms

	Blow speed
	11 mm/s

	Immersion depth aspiration
	-3 mm

	Immersion depth dispense
	3 mm

	Initial stroke
	0 %

	Blow movement
	0 %

	Prewetting
	0 cycles



