Order of analysed strain performance in oxygen gradients left to right:
[bookmark: _GoBack]T1: 
1. KT2440 pS2213 ackA-(pyrK-pyrD B)-(nrdD-nrdG)
2. KT2440 pS2213 nrdD-nrdG
3. KT2440 pS2213 ackA
4. KT2440 pS2213 -
5. Blank medium
T2: 
1. KT2440 pS2213 ackA-(pyrK-pyrD B)-(nrdD-nrdG)
2. KT2440 pS2213 nrdD-nrdG
3. KT2440 pS2213 ackA
4. KT2440 pS2213 -
5. Blank medium
T3: 
1. KT2440 pS2213 –
2. KT2440 pS2213 nrdD-nrdG
3. KT2440 pS2213 ackA
4. KT2440 pS2213 ackA-(pyrK-pyrD B)-(nrdD-nrdG)
5. Blank medium

