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High cell density sequential batch fermentation for enhanced propionic acid production from glucose and glycerol/glucose mixture using Acidipropionibacterium acidipropionici
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Glycerine Tech® 

Chemical composition:
	Glycerine content
	Min. 97%

	Water content
	Max. 1%

	Methanol content
	Max. 0.10%



Organoleptic characteristics:
	Hydroxyl number 
	1800 mg KOH/g

	Colour 
	600 APHA

	Ash content (as sodium) 
	40 ppm

	Saponification value 
	6 mg KOH/g

	Acid value
	2 mg KOH/g



