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Figure S2: Circularity of holes measured using image analysis.
[bookmark: _GoBack]Jitter plot with box and whisker plot overlay displaying the distribution of the circularity of holes as measured by image analysis (shown separately for the different WHOPES hole size categories, d = diameter). The jitter plots show the distribution of circularity (each hole is represented by a dot).  The box in the box and whisker plot show the 75th percentile, median, and 25th percentile, respectively; whereas the whiskers identify the extremes, including the minimum and maximum. 
Circularity indicates the amount of elongation of the hole (1 indicates a perfect circle, values closer to 0 indicate more elongation). The average circularity of all holes was 0.43 (standard deviation = 0.18). Larger holes tended to be less circular than smaller holes (mean circularity = 0.25 for holes with diameter > 25.0 cm; and circularity = 0.46 for holes with a diameter between 0.5 and 2 cm; Table 4). Circularity was significantly associated with hole area (linear regression p-value < 0.0001), with a 0.002 unit decrease in circularity for every 10 cm2 increase in area.
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