Supplemental Table 6. The effect of diesel exhaust exposure status on 9th generation airway dimensions in all study subjects (n=154)a

	Variable
	Non-DET (n=76)
	DET (n=78)
	Ratio (95CI%)
	P

	Wall area (mm2)
	
	
	
	

	LB1+2
	2.3 (1.6, 3.1)
	2.3 (1.8, 3.3)
	
	

	LB9
	2.8 (1.9, 4.1)
	2.9 (2.2, 4.4)
	
	

	RB9
	2.6 (1.8, 4.3)
	2.6 (1.8, 4.1)
	
	

	RB1
	2.4 (1.7, 3.2)
	2.5 (1.9, 3.4)
	
	

	All
	2.5 (2.3, 2.8)
	2.8 (2.6, 3.1)
	1.12 (0.98, 1.28 )
	0.090

	Lumen area (mm2)
	
	
	
	

	LB1+2
	3.0 (2.2, 3.6)
	3.0 (2.4, 3.7)
	
	

	LB9
	3.5 (2.8, 4.9)
	3.9 (3.0, 5.0)
	
	

	RB9
	3.4 (2.7, 4.2)
	3.7 (2.7, 4.3)
	
	

	RB1
	2.8 (2.0, 3.6)
	2.9 (2.3, 3.5)
	
	

	All
	3.0 (2.8, 3.2)
	3.3 (3.1, 3.5)
	1.09 (0.99, 1.19)
	0.067

	Airway area (mm2)
	
	
	
	

	LB1+2
	5.4 (4.4, 6.4)
	5.5 (4.6, 7.1)
	
	

	LB9
	6.7 (5.3, 7.8)
	7.1 (6.2, 8.9)
	
	

	RB9
	6.4 (5.2, 7.8)
	6.5 (5.5, 8.0)
	
	

	RB1
	5.2 (4.1, 6.8)
	5.6 (4.4, 6.8)
	
	

	All
	5.8 (5.5, 6.1)
	6.4 (6.1, 6.7)
	1.10 (1.03, 1.18)
	0.005


[bookmark: _Hlk41559642]Deﬁnition of abbreviations: DETs = diesel engine testers; CI = confidence interval; LB = left bronchus; RB = right bronchus. 
a Linear mixed effects model assessed differences of natural log transformed areas of wall, lumen, and airway between non-DETs and DETs with adjustment of age, BMI, smoking history, CT reconstruction method, and lung lobes. Indices were shown as median (Q1, Q3). Ratio = eβ, 95%CI = e(β ± 1.96×Se) . Descriptive statistics for all were exponentials of least square means and 95%CIs that were calculated based on natural log transformed data using linear mixed effects model with adjustment for covariates listed above and may be regarded as an overall level of airway dimension indices based on the four sampled airways of 9th generation.
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