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Figure S1. Calibration curve of the miniature air flow transmitters. The straight line represents the overall regression (all sensors). 
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Figure S2. Changes in ΔCO2 at different air flux levels when scrubbing the air with soda lime. The data show all ramps (i.e. different pump speeds) normalized from 0 to 1 and averaged every 20 seconds. 
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