Table S1. HPLC conditions for analysis standard compound and PLG extract.
	HPLC Conditions

	Detector
	245nm

	Column
	X-bidge C18 Column (250 mm × 4.6 mm, 5 μm)

	Column Temperature
	25℃

	Injection Volume
	10μL

	Flow rate
	1.0mL / min

	Mobile phase
	Time (min)
	A
	B

	A: Water
B : Methanol
	0.0
	97
	3

	
	12.0
	90
	10

	
	17.0
	80
	20

	
	25.0
	80
	20

	
	35.0
	70
	30

	
	40.0
	60
	40

	
	50.0
	0
	100



[bookmark: _GoBack]
