
Table S1. Mean daily temperatures of the Seine River (°C)

	
	Minimum 
	Maximum

	
2011
	
2.40
	
22.90

	2012
	1.69
	23.96

	2013
	4.26
	25.88

	2014
	6.45
	23.99

	2015
	4.30
	25.53

	2016
	5.20
	23.36

	2017
	3.18
	26.19

	2018
	3.03
	26.46

	2019
	5.20
	26.98

	2020
	6.62
	26.34

	2021
	2.61
	24.28

	2022
	4.69
	25.93

	
	
	

	Legend: Values are means (°C) from five wastewater treatment plants located on the Seine River in the Paris area: Suresnes, Bougival, Andrésy, Méricourt and Alfortville.

	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	









	
	



Table S2. Mean temperature of the Seine River on the day of submersion (°C)

	Temperature

	       Minimum 
     (2000-2022)
	Maximum 
(2000-2022)

	

	
	

	08/06/2013
	17.75
	23.02
	15.88

	17/07/2013
	23.46
	25.35
	17.63

	17/12/2013
	 5.41
	9.17
	3.08

	25/01/2017
	 3.34
	8.80
	3.34

	15/12/2016
	 6.32
	9.35
	3.95

	19/11/2017
	 9.87
	13.61
	7.14

	29/01/2018
	 8.82
	9.09
	3.33

	14/02/2018
	 5.15
	9.85
	1.95

	17/01/2019
	 7.43
	9.04
	3.26

	28/01/2020
	 6.72
	8.92
	3.18



Legend: Values are means (°C) from five wastewater treatment plants located on the Seine River in the Paris area: Suresnes, Bougival, Andrésy, Méricourt and Alfortville.
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Figure S1: French national guidelinesfor extracorporeal cardiopulmonary resuscitation in refractory Cardiac Arrest
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French Resuscitation Council, etal. Guidelines for indications for the use of extracorporeal life supportin refractory cardiacarrest. Ann Fr Anesth Reanim. 2009;28:182-90. [15]




