	M1B

	A. Characteristics of the biogas

	Total Biogas production:
 L/working volume of the bioreactor/d
	36.3 ± 3.3

	Composition of biogas [%]:
	

	methane
	71.9 ± 0.4

	carbon dioxide
	28.0 ± 1.1

	hydrogen
	0.01 ± 0.01 

	hydrogen sulphide
	0.01 ± 0.01 

	Methane production:

	L-CH4/working volume of the bioreactor/d
	25.0 ± 2.0

	L-CH4/g COD
	3.4 ± 0.3

	B. Characteristics of the substrate and effluent after the methanogenic process

	
	Substrate
	Effluent

	COD (g O2/L)
	12.5 ±1.8
	0.6 ± 0.3

	concentration of sulphide (mg/L) 
	<0.05 *
	0.01 ± 0.0

	pH
	4.91 ± 0.12
	7.40 ± 0.1

	Redox potential in the UASB bioreactor (mV) **
	
	(-310)–(-320)
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* – the limit of quantification
** – according to hydrogen electrode



