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Additional Table S1. Comparison between batch and SCF operation under similar conditions.
	Operation mode
	Cycle time, (h)
	Ethanol produced (g/L)
	Fermentation efficiency
(%)
	Annual ethanol productivity*
(ton/year)

	Batch
	23.4
	21.5 ± 0.1
	81.1 ± 0.8
	580 ± 3

	SCF 
  Cycle 1
  Cycle 4
  Cycles 2,3,5-21
	
22.6
10.7
6.7-7.5
	
22.4 ± 0.5
10.5 ± 0.3
9.5-11.2 
	80.8-91.2
	1020 ± 16


*Based on a fermenter of volume 105 L.
Mean values from triplicate analysis ± standard deviation.
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