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	Acetonitrile elution gradient setting
	Parameter settings (DIA)

	Time (min)
	Flow（µL/min)
	%B
	Name of the Properties
	Properties

	0.000
	0.300
	4.0
	Runtime
	0 to 60 min

	1.800
	0.300
	4.5
	Full-scan scan range 
	400-1200 m/z

	2.000
	0.300
	5.0
	Full-scan Orbitrap Resolution
	120000

	47.000
	0.300
	20.0
	Full-scan AGC Target
	Custom

	57.000
	0.300
	35.0
	Full-scan Normalized AGC Target
	300%

	57.500
	0.300
	55.0
	Full-scan Maximum IT
	50 ms

	57.500
	Column Wash
	
	HCD collision energy
	30%

	58.000
	0.800
	99.0
	DIA Window Type
	Auto

	
	
	
	Orbitrap Resolution
	30000

	
	
	
	AGC Target
	Custom

	
	
	
	Normalized AGC Target
	2000%

	
	
	
	Maximum IT 
	Custom




